**Specifications -**Ansal Paradise Crystal Apartments

* Living/Dinning
	+ Floor – Imported/Indian Marble
	+ Walls – Plastic Emulsion paint
	+ Ceiling – Oil bound distemper with POP Moulding & Cornice
* Master/Bedroom
	+ Floor – Laminated/Wooden Flooring
	+ Walls – Plastic Emulsion paint
	+ Ceiling - Oil bound distemper with POP Moulding & Cornice
* Other Bedroom
	+ Floor – Vitrified Tile/Wooden Flooring
	+ Walls – Plastic Emulsion paint
	+ Ceiling - Oil bound distemper with POP Moulding & Cornice
* Doors
	+ Internal Door – Painted Hardwood Frame with painted Moulded skin Doors
	+ Entrance Door – Veneered and polished flush shutter/Moulded Skin Door/Steel Shutter
* Toilets
	+ Walls – Ceramic Tiles Up to 7ft. Height
	+ Floor – Ceramic Tiles
	+ Counters – Marble/Granite
	+ Fitting/Fixtures – Single lever C.P fitting, Wall hung WC, Towel Ring, Towel Rod, Paper Holder, Bathing cubical in master bedroom toilet. Exhaust Fans fitted.
* Kitchen
	+ Walls – Ceramic tile up to 2ft. above counter and oil bound distemper in the balance area.
	+ Floor – Ceramic Tiles
	+ Counter – Polished Granite Counter
	+ Fitting/Fixtures – CP fittings, single bowl stainless steel sink with drain board. Exhaust Fan fitted. Water Purified.
* Balcony
	+ Floor – Anti Skid Ceramic Tile
	+ Walls & Ceiling – Texture Paint/Oil Bound Distemper
* External Finishes
	+ Texture Paint finish/Semi permanent finish
* Electrical Works
	+ Electrical Work with copper wires in concealed PVC Conduits, Provision Shall be made for sufficient light & Power Points.
* Switches & Sockets
	+ Telephone & TV points in all Bedroom, Drawing/Dining Room
* Windows
	+ UPVC/Aluminium anodized windows with sliding glass shutter