**Specifications -**Ansal Paradise Crystal Apartments

* Living/Dinning
  + Floor – Imported/Indian Marble
  + Walls – Plastic Emulsion paint
  + Ceiling – Oil bound distemper with POP Moulding & Cornice
* Master/Bedroom
  + Floor – Laminated/Wooden Flooring
  + Walls – Plastic Emulsion paint
  + Ceiling - Oil bound distemper with POP Moulding & Cornice
* Other Bedroom
  + Floor – Vitrified Tile/Wooden Flooring
  + Walls – Plastic Emulsion paint
  + Ceiling - Oil bound distemper with POP Moulding & Cornice
* Doors
  + Internal Door – Painted Hardwood Frame with painted Moulded skin Doors
  + Entrance Door – Veneered and polished flush shutter/Moulded Skin Door/Steel Shutter
* Toilets
  + Walls – Ceramic Tiles Up to 7ft. Height
  + Floor – Ceramic Tiles
  + Counters – Marble/Granite
  + Fitting/Fixtures – Single lever C.P fitting, Wall hung WC, Towel Ring, Towel Rod, Paper Holder, Bathing cubical in master bedroom toilet. Exhaust Fans fitted.
* Kitchen
  + Walls – Ceramic tile up to 2ft. above counter and oil bound distemper in the balance area.
  + Floor – Ceramic Tiles
  + Counter – Polished Granite Counter
  + Fitting/Fixtures – CP fittings, single bowl stainless steel sink with drain board. Exhaust Fan fitted. Water Purified.
* Balcony
  + Floor – Anti Skid Ceramic Tile
  + Walls & Ceiling – Texture Paint/Oil Bound Distemper
* External Finishes
  + Texture Paint finish/Semi permanent finish
* Electrical Works
  + Electrical Work with copper wires in concealed PVC Conduits, Provision Shall be made for sufficient light & Power Points.
* Switches & Sockets
  + Telephone & TV points in all Bedroom, Drawing/Dining Room
* Windows
  + UPVC/Aluminium anodized windows with sliding glass shutter